PolySketch — Field Interface
Standard Operating Procedure
Component Drawing for the Field, Office & Shop Floor
polyfabpro.com  ·  Designer & Fabricator Portals
✏️  PolySketch lets you draw a component anywhere — on your phone at the job site, on a tablet in the field, or at a desk in the office — and route it directly to the right person for approval.
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1.  What Is PolySketch?

PolySketch is a component drawing tool built into both the Designer and Fabricator portals of PolyFab Pro. It is designed to capture the exact shape, dimensions, and angles of a custom component — directly from wherever you are — and send it to the right person for review and approval.
Unlike a general-purpose drawing app, PolySketch is purpose-built for fabrication communication. Every sketch is tied to a specific job and location, saved automatically, and routed to the correct recipient based on who is drawing it.
💡  When field conditions change and a component needs to be redrawn, PolySketch is where that correction happens — before it becomes a costly mistake.
2.  Who Uses It & When

	Role
	When to Use PolySketch

	Project Manager (PM)
	When a component needs custom fabrication detail. Sketch goes to the Fabricator OM for production.

	Operations Manager (OM)
	When the shop needs to confirm field dimensions with the PM. Sketch goes to the PM for approval.

	Field Technician
	When site conditions differ from original specs. Sketch goes to both PM and OM simultaneously.



✅  You do not need to be a trained drafter to use PolySketch. The tools are simple and designed for fast, accurate capture.
3.  Accessing PolySketch

PolySketch lives inside both the Designer and Fabricator portals. It is not a separate app — you access it from the portal you are already logged into.
From the Designer Portal
Log in at polyfabpro.com/designer
Click PolySketch in the top navigation bar.
From the Fabricator Portal
Log in at polyfabpro.com/fabricator
Click the ✏️ PolySketch button in the top navigation bar, or select it from the sidebar.
📱  PolySketch works on any device — phone, tablet, or desktop. For field use, a phone or tablet is recommended.
4.  Selecting a Job & Location

Every sketch is tied to a specific job and location. This keeps your sketches organized and makes it easy to reload them later.
On the PolySketch home screen, select a job from the Job dropdown.
In the Location / Section field, type the name of the specific area — for example: 'North Elevation - Window 3' or 'Roof Parapet East'.
The job and location together create a unique save slot for your sketch.
📌  Be as specific as possible with the location name. This is what you and the fabricator will use to find the sketch again.
5.  Starting a New Sketch

Once a job and location are selected, you can start a new sketch or load an existing one.
Click New Sketch. The drawing canvas opens.
The canvas starts blank. You are now in drawing mode.
⚠️  If a sketch already exists for this job + location, clicking New Sketch will start fresh. Use Load Sketch if you want to continue a previous sketch.
6.  The Drawing Tools

The PolySketch toolbar gives you everything you need to capture a component accurately.
	Tool
	What It Does

	Segment tool
	Draw a straight line segment. Click to set start point, click again to set end.

	Angle pad
	Enter an exact angle (in degrees) for the next segment direction.

	Dimension pad
	Enter an exact length for the current segment.

	Hem overlay
	Display standard hem profiles as a reference overlay.

	Erase
	Remove the last drawn point or segment.

	Clear
	Remove all segments and start the canvas fresh.

	Undo / Redo
	Step backward or forward through drawing actions.

	Zoom
	Pinch to zoom on touch devices; scroll wheel on desktop.



💡  For the most accurate sketches, use the angle pad and dimension pad to enter exact values rather than drawing freehand.
6a.  Managing Angle Labels

After placing an angle label on the sketch, you can remove it from the drawing without losing the underlying degree value. The angle is still used in the clean profile output — only the visible label is hidden. You can restore it at any time.
Removing an Angle Label
Switch to the Select tool (S).
Tap the angle° label you want to remove.
The angle pad opens showing the current value.
Tap 🗑 Remove Label. The label disappears from the sketch and the final drawing.
⚠️  Removing the label does not change the angle — it only hides it. The degree value is preserved in the saved sketch data.
Restoring a Removed Angle Label
Switch to the Select tool (S).
Tap the junction where the angle label was (the corner between two segments).
The angle pad opens. The previous degree value is pre-filled.
Confirm with ✓ (or type a new value first). The label reappears on the sketch.
📋  You can also use this flow to change an angle value — open the angle pad on any junction and type the corrected degrees before confirming.
7.  Saving a Sketch

Sketches are saved to your device's local storage, keyed to the job and location you selected. They persist between sessions so you can return and continue at any time.
Click the Save button in the sketch toolbar.
A confirmation message appears: 'Sketch saved.'
The sketch is now accessible any time you select the same job and location.
💾  Save frequently while drawing — especially before sending. PolySketch auto-saves are not guaranteed on all devices.
8.  Loading a Saved Sketch

If you have previously saved a sketch for a job and location, you can load it to view, revise, or resend.
Select the same job from the dropdown.
Type the same location name in the Location / Section field.
Click Load Sketch.
The saved sketch loads on the canvas. You can edit and re-save as needed.
📂  Location names are case-sensitive. Use the same spelling and capitalization you used when the sketch was first saved.
9.  Sending a Sketch via Email

When a sketch is ready, you send it via your email client. PolySketch automatically determines the To and CC recipients based on your role.
Click the Send button (or 'Send to PM' / 'Send to Fabricator' depending on your portal).
The email modal opens with pre-filled fields.
Review the To, CC, subject, and message body.
Edit the CC field if needed.
Click Open Email Client.
Your device's email app opens with all fields pre-filled and ready to send.
📧  PolySketch opens your email client — it does not send the email on your behalf. You review it and click Send in your email app.
10.  How Routing Works

PolySketch automatically routes the sketch to the correct person based on which portal you are using.
	Who Sends
	Portal Used
	Email Goes To
	CC

	Project Manager
	Designer Portal
	Fabricator OM
	PM's own email

	Operations Manager
	Fabricator Portal
	Project Manager
	OM's own email

	Field Technician
	Either portal
	PM + Fabricator OM
	Field tech's email



💡  You can always edit the CC field before sending if additional recipients need to be included.
11.  Field Technician Workflow

Field technicians typically encounter changed conditions on site — a window rough opening that's out of spec, a parapet profile that differs from the drawings, or a custom condition not covered by the original takeoff.
Step-by-step
Open PolySketch on your phone or tablet.
Log in to the Designer or Fabricator portal (whichever your shop uses).
Select the job and type the specific location where the condition exists.
Tap New Sketch and draw the component as it actually exists in the field.
Use the angle pad and dimension pad for precise measurements.
Save the sketch.
Tap Send. Both the PM and the Fabricator OM receive the sketch.
Wait for confirmation before fabrication proceeds.
⚠️  Never proceed with fabrication based on a field condition that hasn't been confirmed. Send the sketch and wait for approval.
12.  Quick Reference Card

	Task
	Steps

	Open PolySketch
	Log in → Click PolySketch in nav

	Select a job
	Choose from Job dropdown

	Set a location
	Type in Location / Section field

	New sketch
	Click New Sketch → draw on canvas

	Enter exact angle
	Click Angle Pad → type degrees → confirm

	Enter exact dimension
	Click Dimension Pad → type length → confirm

	Save sketch
	Click Save → 'Sketch saved' confirms

	Load saved sketch
	Same job + location → Click Load Sketch

	Send sketch
	Click Send → review email modal → Open Email Client → Send

	Re-send revised sketch
	Load → edit → Save → Send again
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